Eightdog Race Timer

|  |  |
| --- | --- |
| **Handicap Racing****Before Starting**The unit should have been left in the Handicap Racing mode with 5, 4, 1, Go programmed.If PSt on lower line is NOT Zero then Pursuit mode is enabled and should be set to ZERO. See RED below.The number of Fleets (FL) should normally be set to 1. If not see RED below.You should see 5,4,1,0 (FL or PSt) on the lower screen and NOTHING on the upper. If there is something on the upper press MENU until you just have 5,4,1, 0 (FL or PSt)on the lower menu.**Start Handicap Race**Press START. The unit will count down from 6 minutes. At 5, 4, 1 and 0 the unit will beep. Before each mark there is a 10 second warning beep so you can be ready to hoist/drop the appropriate flags. As each boat passes the Finish press the Finish button or Remote control.**Individual Recall:** Press remote button or ‘Overide’ button on unit.**General Recall**: Press **Recall** button on unit within 45 seconds of the start of the race. A double horn will sound. **Press Menu +Log** for 5 seconds before the next minute mark to Cancel the programme, and start again.**Shorten Course:** A press on the remote switch or ‘Override’ button**FINISH**As each boat passes the Finish press the Finish button or Remote control.**Press Menu +Log** for 5 seconds to Cancel the programmeSwitch off | **Pursuit Racing**Please revert the unit to handicap racing at the end of the race.**Set Pursuit Racing**Press **MENU** until PUrST (Pursuit) is seen on top line.Press **– (minus**) or **+ (plus)** until Pursuit interval is set to: 30 for half Pursuit 60 for full PursuitPress **MENU** until FLEETS is shown **PRESS – (minus)** to set the number of fleets to 200 . (Scrolls to 200 from 1 if you press minus). This will give you 200 ‘beeps’ at the appropriate interval.Press MENU until 5,4,1,0 is shown on lower screen.**The Race**Press **START** – the unit will count down from 6 minutes to 0. The unit will then count down 4, 1, Go. Get the number board ready with the correct number for the first boat to start and display the number during the last 1 minute (or 30 secs). On the ‘Go’ turn the number over.After that the unit will then beep every 30 seconds or 60 seconds as programmed.When the last boat has gone over the start line press **Menu for 2 secs** to stop the Beep, counter will keep counting up.When the race is completed Sound Horn using Remote Switch or Press Finish button. Then cancel the timer by Pressing MENU and LOG together for 5 seconds.Revert the unit to Handicap Racing.Press **MENU** until PUrST (Pursuit) is seen on top line.Press **– (minus)** until Pursuit interval is set to 0Press **MENU** until FLEETS is shown The number of Fleets should be set to 1. **PRESS + (plus)** to set the number of fleets to 1 or required number. (Scrolls round to 1 after 200).Press MENU until 5,4,1,0 is shown.Switch off. |